{"text_format":"1","workbook":"xlsx","n_sheets":18,"sheets":["Print PDF","Front-Page","1-Fluid-Analysis-Results","2-SSF","2-SSF-Compositions","3-CCE","3-CCE-plots","4-DLE","4-DLE-Compositions","4-DLE-plots","5-Sep-Test","5-Sep-Test-Compositions","6-CVD","6-CVD-Compositions","6-CVD-Plots","7-Visc","7-Visc-plots","UNITS"],"not_rendered":{"charts":22,"images":0,"macros":1,"external_links":0,"defined_names":29,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Print PDF","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[[10,3,12,7],[13,3,13,7],[14,3,14,7]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Click the button to convert the PVT report to PDF format"]
[]
[]
[]
[null,null,null,"Macros should be enabled in the workbook"]

{"sheet":"Front-Page","index":1,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[[26,3,26,4],[4,1,4,6],[8,1,8,6],[5,1,5,6],[22,3,25,4]]}
[]
[]
[]
[]
[null,"Simulated PVT Study"]
[null,"Generated with whitson+"]
[]
[]
[null,"Oil Sample"]
[]
[]
[null,null,null,"Well:","SPE-DATA-REPOSITORY-DATASET-1-WELL-4-KITE"]
[null,null,null,"Field:","Jesus - Support"]
[]
[]
[]
[null,null,null,"calcid:","787d73ff-40e1-4251-83c2-77a180a18a56"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"TODAY()","v":null}]

{"sheet":"1-Fluid-Analysis-Results","index":2,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[[2,5,3,6]]}
[null,"1. Fluid Analysis Results"]
[]
[null,"Table 1: Reservoir Conditions",null,null,null,"Table 2: Composition of Reservoir Fluid"]
[null,"Reservoir Pressure",6600,{"$f":"p_unit","v":null}]
[null,"Reservoir Temperature",237.716614,{"$f":"T_unit","v":null},null,"Component","mol%"]
[null,null,null,null,null,"N2",1.55176106315041e-152]
[null,"Table 3: Fluid Properties at Reservoir Conditions",null,null,null,"CO2",1.54453459883206e-152]
[null,"Density",43.97889282553894,{"$f":"dens_unit","v":null},null,"H2S",1.532047836168863e-152]
[null,"Viscosity",0.5360434501724228,{"$f":"visc_unit","v":null},null,"C1",37.53182971265226]
[null,null,null,null,null,"C2",10.03824872561911]
[null,null,null,null,null,"C3",7.660458312278275]
[null,"Table 4: Fluid Properties at Saturation Conditions",null,null,null,"I-C4",1.040774152348906]
[null,"Bubble Point Pressure",2875.456564497617,{"$f":"p_unit","v":null},null,"N-C4",4.435359996117386]
[null,"Density",41.38650451747259,{"$f":"dens_unit","v":null},null,"I-C5",1.735451516912192]
[null,"Viscosity",0.3255769851515713,{"$f":"visc_unit","v":null},null,"N-C5",2.201312168514337]
[null,"Formation Volume Factor (Bo) ** ",1.46986190452016,{"$f":"sep_bo_unit","v":null},null,"C6",3.260355502311429]
[null,"Solution GOR (Rs) **",749.9900000000009,{"$f":"sep_gor1_unit","v":null},null,"C7",3.279852727795084]
[null,null,null,null,null,"C8",4.027755489669103]
[null,"Table 5: Stock Tank Oil Properties",null,null,null,"C9",2.71630833051654]
[null,"Density **",52.11309248027182,{"$f":"dens_unit","v":null},null,"C10",2.239108688063584]
[null,"API Gravity **",37.84199162711101,"API",null,"C11",1.740109391079883]
[null,null,null,null,null,"C12",1.401485677341801]
[null,null,null,null,null,"C13",1.448389965083075]
[null,null,null,null,null,"C14",1.240948338700065]
[null,null,null,null,null,"C15",1.167626236252134]
[null,"** Properties from multi-stage separator test",null,null,null,"C16",0.9239646628646859]
[null,null,null,null,null,"C17",0.8584486827831632]
[null,null,null,null,null,"C18",0.8430331254520764]
[null,null,null,null,null,"C19",0.7568991932822037]
[null,null,null,null,null,"C20",0.6175819427473597]
[null,null,null,null,null,"C21",0.5723953658476033]
[null,null,null,null,null,"C22",0.5243183927924105]
[null,null,null,null,null,"C23",0.4828893387341429]
[null,null,null,null,null,"C24",0.4418456716427802]
[null,null,null,null,null,"C25",0.4157357332567749]
[null,null,null,null,null,"C26",0.3897221415676047]
[null,null,null,null,null,"C27",0.370356467768754]
[null,null,null,null,null,"C28",0.3474259684574315]
[null,null,null,null,null,"C29",0.3254589355074963]
[null,null,null,null,null,"C30+",4.964549446040365]
[null,null,null,null,null,"Total",100]

{"sheet":"2-SSF","index":3,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[[8,1,9,7]]}
[null,"2. Single Stage Flash (SSF)"]
[]
[null,"Table 6: Single Stage Flash of Reservoir Fluid at Standard Conditions"]
[null,"Pressure","Temperature","GOR","Separator Volume Factor","Specific Gravity for Flashed Gas","Oil Molecular Weight","Oil Density","Stock Tank Oil Gravity"]
[null,{"$f":"p_unit_p","v":null},{"$f":"T_unit_p","v":null},{"$f":"gor_unit_p","v":null},{"$f":"sep_bo_unit_p","v":null},"(air=1)","(-)",{"$f":"dens_unit_p","v":null},"(API)"]
[null,2875.456564497617,237.716614,0,1.534781767510421,"-",98.48934743845385,41.38650451747259,"-"]
[null,14.69594300599296,59.99999999999998,841.9521783889877,1,0.9447889143711167,211.0146163113071,52.70568085649765,35.93802047610015]
[]
[null,"It is common for the PVT laboratory to use a higher temperature for the SSF and the main reason for that is so the final oil is thermally stable at room temperature. "]
[]
[]
[null,"Table 6b: Single Stage Flash of Reservoir Fluid to 1 atm and 140 F"]
[null,"Pressure","Temperature","GOR","Separator Volume Factor","Specific Gravity for Flashed Gas","Oil Molecular Weight","Oil Density","Stock Tank Oil Gravity"]
[null,{"$f":"p_unit_p","v":null},{"$f":"T_unit_p","v":null},{"$f":"gor_unit_p","v":null},{"$f":"sep_bo_unit_p","v":null},"(air=1)","(-)",{"$f":"dens_unit_p","v":null},"(API)"]
[null,2875.456564497617,237.716614,0,1.677814042373783,"-",98.48934743845385,41.38650451747259,"-"]
[null,14.69594300599296,140,1003.178555960732,1.020959787821235,1.136874455252429,238.9703119827727,52.50953018960496,"-"]
[null,14.69594300599296,59.99999999999998,0,1,"-",238.9703119827726,53.61011880097185,33.11323100625313]

{"sheet":"2-SSF-Compositions","index":4,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[[3,6,3,8],[3,1,4,1],[3,3,3,5]]}
[null,"2. Compositional Analysis of Reservoir Fluid from SSF"]
[]
[null,"Table 7: Compositional Analysis Data"]
[null,"Component","MW","mol-%",null,null,"mass-%"]
[null,null,"-","Flashed Gas","Flashed Liquid","Reservoir Fluid","Flashed Gas","Flashed Liquid","Reservoir Fluid"]
[null,"N2",28.014,2.530110290205169e-152,3.925384369996882e-155,1.55176106315041e-152,2.590128136193108e-152,5.211284396473354e-156,4.413780327893907e-153]
[null,"CO2",44.01,2.496513052249561e-152,3.841983440824247e-154,1.54453459883206e-152,4.015058541283506e-152,8.012984796333978e-155,6.901758358900352e-153]
[null,"H2S",34.082,2.427598101236641e-152,1.152074952344731e-153,1.532047836168863e-152,3.023489979307444e-152,1.86077245321651e-154,5.301614409105166e-153]
[null,"C1",16.043,61.07202986106483,0.2891349082278303,37.53182971265226,35.80425246421154,0.02198232242763615,6.11358649174062]
[null,"C2",30.07,15.99515360503099,0.6138942594620411,10.03824872561911,17.57634285025003,0.08748114564154211,3.064799869528969]
[null,"C3",44.097,11.42693248403723,1.701560461657185,7.660458312278275,18.41388295544488,0.3555853759769923,3.429845348580757]
[null,"I-C4",58.123,1.361278330787522,0.5337079750913979,1.040774152348906,2.891356386887255,0.1470073930351482,0.6142077049985284]
[null,"N-C4",58.123,5.317413866695479,3.039872154217433,4.435359996117386,11.29419178831592,0.8373187237367319,2.617505707563228]
[null,"I-C5",72.15000000000001,1.436769624978997,2.207992891868434,1.735451516912192,3.78817597730584,0.7549556989610828,1.271333704626892]
[null,"N-C5",72.15000000000001,1.550570459661907,3.23084355340084,2.201312168514337,4.088222401345082,1.104688227065624,1.61260762802352]
[null,"C6",84.021,1.168587307456708,6.56971922867845,3.260355502311429,3.588026842308127,2.615905897714887,2.781400595946613]
[null,"C7",97.791,0.437275320912321,7.777063548223297,3.279852727795084,1.562645719745606,3.604142853887947,3.256596641624009]
[null,"C8",111.727,0.1801080954937281,10.11507661323124,4.027755489669103,0.7353566832755677,5.355681916835681,4.569113810764878]
[null,"C9",125.706,0.0395496469644766,6.951179150990209,2.71630833051654,0.1816792342513156,4.140968723537437,3.466935906030738]
[null,"C10",139.695,0.01058708216894718,5.764828499710833,2.239108688063584,0.05404603250496869,3.816407277110276,3.1758996918373]
[null,"C11",153.684,0.002686118882243829,4.48886786656483,1.740109391079883,0.01508552947239636,3.269286181519281,2.715288288673415]
[null,"C12",167.669,0.000712184460275024,3.617634195901963,1.401485677341801,0.004363670400006472,2.874517029179764,2.385899674896976]
[null,"C13",181.651,0.0002444867403141011,3.739485186971561,1.448389965083075,0.001622929952472211,3.219119298809313,2.671369974420008]
[null,"C14",195.628,7.022094089499495e-05,3.20412812212726,1.240948338700065,0.0005020007102264557,2.970491747125121,2.464878161111993]
[null,"C15",209.601,2.235721359242295e-05,3.014879642992047,1.167626236252134,0.0001712449206346405,2.994682544258025,2.484894388173496]
[null,"C16",223.57,6.045263062808576e-06,2.385749549582211,0.9239646628646859,4.938958799325293e-05,2.527701806272999,2.097392104316096]
[null,"C17",237.537,1.937463911374495e-06,2.216587948388868,0.8584486827831632,1.681789207986234e-05,2.495190431357021,2.070409948544842]
[null,"C18",251.5,6.629636998897137e-07,2.176785621723618,0.8430331254520764,6.093045360295718e-06,2.59442494284769,2.15274886640599]
[null,"C19",265.461,2.095683185165333e-07,1.954380848939925,0.7568991932822037,2.032979630384701e-06,2.458653829813595,2.04009085219543]
[null,"C20",279.42,6.080220391782267e-08,1.594651525886674,0.6175819427473597,6.208454207960003e-07,2.111595571682579,1.752115847353981]
[null,"C21",293.377,2.024391345121427e-08,1.477975820958084,0.5723953658476033,2.17033716570533e-07,2.054853450462073,1.705033484471106]
[null,"C22",307.333,6.734041408075098e-09,1.353836812738259,0.5243183927924105,7.562957331150953e-08,1.971800515256497,1.636119527675486]
[null,"C23",321.288,2.275903228195573e-09,1.246863309585788,0.4828893387341429,2.672113918938935e-08,1.898457206486566,1.575262237981287]
[null,"C24",335.242,7.722933497070581e-10,1.140884905257596,0.4418456716427802,9.461225428491325e-09,1.812540496455992,1.503972058962342]
[null,"C25",349.196,2.725151352718676e-10,1.07346671792177,0.4157357332567749,3.477495368460587e-09,1.776418575092442,1.473999563262938]
[null,"C26",363.15,9.685103344955147e-11,1.006297305831905,0.3897221415676047,1.285277722474928e-09,1.731808312622914,1.436983789528268]
[null,"C27",377.103,3.527164843661403e-11,0.9562934100921979,0.370356467768754,4.860628363422098e-10,1.708986420608792,1.418047115727676]
[null,"C28",391.056,1.282539788831777e-11,0.8970848170796933,0.3474259684574315,1.832805896210802e-10,1.662493368281042,1.379469080206774]
[null,"C29",405.01,4.710440375186611e-12,0.8403639800646675,0.3254589355074963,6.971623571180838e-11,1.612949005692897,1.338359192117319]
[null,"C30+",550,8.345984314628836e-15,12.81890916663193,4.964549446040365,1.677439733713133e-13,33.41190371024442,27.7238327427085]
[null,"Total","-",99.99999999999997,100,100,99.99999999999997,100,99.99999999999997]

{"sheet":"3-CCE","index":5,"n_rows":39,"n_cols":9,"rows_kept":39,"cut":false,"hidden":false,"merged":[]}
[null,"3. Constant Composition Expansion (CCE)"]
[]
[null,"Table 8: Constant Composition Expansion (CCE) at Reservoir Temperature"]
[null,null,"Pressure","Vliq/Vtot","Vliq/Vsat","Rel Volume","Oil Viscosity","Density","Compressibility"]
[null,null,{"$f":"p_unit_p","v":null},"(%)","(%)","Vr=V/Vsat",{"$f":"visc_unit_p","v":null},{"$f":"dens_unit_p","v":null},{"$f":"comp_unit_p","v":null}]
[null,"Pres",6600,100,94.1053806917101,0.9410538069171009,0.5360434501724228,43.97889282553894,11.80255878609131]
[null,null,6400,100,94.328043146593,0.9432804314659301,0.5248022832276478,43.87508013195482,11.9945425279933]
[null,null,6200,100,94.5579816869547,0.9455798168695471,0.5135478442787217,43.7683882197142,12.36089779636707]
[null,null,6000,100,94.79560691428031,0.9479560691428031,0.5022812015234231,43.65867350255657,12.74699485592321]
[null,null,5800,100,95.04136365229519,0.9504136365229519,0.4910034539447519,43.54578146509279,13.15443098701783]
[null,null,5600,100,95.2957348040663,0.952957348040663,0.4797157301790291,43.42954551173325,13.58498024368711]
[null,null,5400,100,95.55924576560926,0.9555924576560927,0.4684191869452471,43.30978565798512,14.04061869901143]
[null,null,5200,100,95.83246949509508,0.9583246949509509,0.45711500693965,43.18630703718937,14.52355416594109]
[null,null,5000,100,96.11603235797425,0.9611603235797425,0.4458043960776226,43.05889819019248,15.03626135202983]
[null,null,4800,100,96.41062089492246,0.9641062089492246,0.4344885799372938,42.9273290985021,15.58152364971008]
[null,null,4600,100,96.7169896930407,0.967169896930407,0.4231687992242734,42.7913489127656,16.16248307877523]
[null,null,4400,100,97.03597058332444,0.9703597058332444,0.4118463040322402,42.65068331741389,16.7827003093119]
[null,null,4200,100,97.36848344189957,0.9736848344189957,0.4005223466168016,42.50503145832419,17.44622723559295]
[null,null,4000,100,97.71554894279649,0.9771554894279648,0.3891981723257738,42.3540623424227,18.15769529231906]
[null,null,3800,100,98.07830370144521,0.980783037014452,0.3778750082322041,42.19741059496195,18.92242367225892]
[null,null,3600,100,98.45801836807499,0.98458018368075,0.3665540488889868,42.03467142996265,19.74655291684826]
[null,null,3400,100,98.8561193892823,0.9885611938928229,0.3552364384545507,41.86539464946831,20.63721115158076]
[null,null,3200,100,99.27421536915216,0.9927421536915215,0.3439232482116942,41.68907743423252,21.60272273688263]
[null,null,3000,100,99.714129250103,0.99714129250103,0.3326154481930592,41.50515561708106,22.46234928530975]
[null,"Psat",2875.456564497617,100,100,1,0.3255769851515713,41.38650451747259]
[null,null,2800,98.23223999374865,99.13070599109986,1.009146345409698,0.333566494760603]
[null,null,2600,93.44932414778229,96.92578747677217,1.037201588782944,0.3558859721892654]
[null,null,2400,88.46582532668789,94.84075166834609,1.072060892645457,0.3800837164226184]
[null,null,2200,83.20947950547884,92.84848530648654,1.1158402366929,0.4064868881652591]
[null,null,2000,77.6107404111246,90.92437465741766,1.171543708715665,0.4355035753110416]
[null,null,1800,71.60379741348299,89.04468638376585,1.24357491641915,0.4676567113481742]
[null,null,1600,65.12906589905629,87.18473555859563,1.338645570223953,0.503638889073154]
[null,null,1400,58.13763428804074,85.31642979608792,1.467490565119847,0.5444054944448279]
[null,null,1200,50.59848732687568,83.40443684474718,1.648358305771849,0.5913426744039726]
[null,null,1000,42.50988930675879,81.39935318206309,1.914833336654234,0.6465938263097619]
[null,null,800,33.91735402602699,79.22380709263783,2.335789726752985,0.7137609691943383]
[null,null,600,24.94283992046042,76.73928207706543,3.076605644015571,0.7996440699555445]
[null,null,400,15.83578588787705,73.64585843249196,4.650597005663665,0.9196595592432332]
[null,null,300,11.36910878654696,71.64652870868792,6.301859719511794,1.004423090261304]

{"sheet":"3-CCE-plots","index":6,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[null,"Figure 1: Plots Constant Composition Expansion (CCE)"]
[]
[null,null,null,"(A) Vliq/Vtot",null,null,null,null,"(B) Vliq/Vsat"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(C) Relative Volume",null,null,null,null,"(D) Density"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(E) Compressibility "]

{"sheet":"4-DLE","index":7,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[[2,1,2,19]]}
[null,"4. Differential Liberation Expansion (DLE) "]
[]
[null,"Notes:\n** Z factor and gas gravity for incipient gas at the bubblepoint.\n*** Simulated depletion down to atmospheric pressure is a single flash calculation. Laboratory depletion to atmospheric pressure will likely be a bleeding process that will result  in less shrinkage than a single flash. Therefore, the simulated final stage flash leads to Rsd and Bod values that will be greater than laboratory values (at all pressures). This discrepancy can become significant at higher temperatures and for lighter oils (higher API)."]
[null,"Table 9: Differential Liberation Expansion (DLE) at Reservoir Temperature"]
[null,null,"Pressure","Solution Gas Oil Ratio","Relative Oil Volume","Oil Density","Gas Z Factor","Incremental Gas Gravity"]
[null,null,null,"Rsd","Bod",null,"Z"]
[null,null,{"$f":"p_unit_p","v":null},{"$f":"dle_gor_unit_p","v":null},{"$f":"dle_bo_unit_p","v":null},{"$f":"dens_unit_p","v":null},"-","(air=1)"]
[null,"Psat**",2875.456564497617,1087.938236975172,1.732569186663018,41.38650451747259,0.8491571785774881,0.8392414433853175]
[null,null,2800,1058.879292670233,1.717508066523306,41.55732332417751,0.8478525941733578,0.8352452781627223]
[null,null,2600,984.7258218948429,1.679156937891605,42.01074551857147,0.8454873702535382,0.8257628159407975]
[null,null,2400,914.1589252002707,1.642661596237435,42.46642726068208,0.8446854563516287,0.8179686356017165]
[null,null,2200,846.7944450910551,1.607787273488484,42.92507168644585,0.8454227257395582,0.8119940292526658]
[null,null,2000,782.2949114870983,1.574325911839442,43.38738803282296,0.8476708058224761,0.8080404617410419]
[null,null,1800,720.3540559202005,1.542085619387276,43.85415920739765,0.8513963533771344,0.8064158071157999]
[null,null,1600,660.6804682152267,1.510878978347699,44.32634590440797,0.856560801002489,0.8075965283123023]
[null,null,1400,602.9769869250621,1.480507545665684,44.80526163410426,0.8631207049502494,0.812340108722324]
[null,null,1200,546.9091647933553,1.450737205964592,45.2928935916965,0.8710289288528109,0.8219024117663392]
[null,null,1000,492.0470956337158,1.42125162397037,45.79255322313573,0.8802374307297383,0.8384954924459515]
[null,null,800,437.7364241100177,1.391547718589925,46.31037954715764,0.8907048955573962,0.8663669594411356]
[null,null,600,382.7449502500554,1.360646941554035,46.85952016266264,0.9024261011006243,0.9147708697652871]
[null,null,400,323.9552713320747,1.326015934897648,47.47568380766109,0.9156044126822763,1.008212387656154]
[null,null,200,248.1911447264873,1.276618504886375,48.31510130095698,0.9324588756979277,1.236542743141547]
[null,"***",14.69594300599296,0,1.051152077373118,51.22242700328988,0.9830874979447422,2.322941792772494]
[null,"Residual",14.69594300599296,0,1,53.84256055260105]

{"sheet":"4-DLE-Compositions","index":8,"n_rows":40,"n_cols":19,"rows_kept":40,"cut":false,"hidden":false,"merged":[[2,1,2,19]]}
[null,"Table 10: Compositions from Differential Liberation Expansion (DLE) Test"]
[null,"Removed gas compositions, mol-%. *Residual oil at standard conditions (1 atm, 60 F)"]
[null,"Notes:\n1. First column is the incipient gas at bubblepoint.\n2. Last column (*) is stock tank oil at standard conditions (1 atm, 60 F)"]
[null,"Pres (psia)",2875.46,2800,2600,2400,2200,2000,1800,1600,1400,1200,1000,800,600,400,200,14.7,"14.7*"]
[null,"N2",4.510563243859107e-152,4.478467829324267e-152,4.379977504298924e-152,4.252341305419302e-152,4.092062302419154e-152,3.895631784961658e-152,3.659660531818971e-152,3.38106488749099e-152,3.057333460521724e-152,2.68692272793259e-152,2.269880336269843e-152,1.808920148658537e-152,1.311537820060462e-152,7.951513111289866e-153,3.060812660569313e-153,1.943305469974881e-154,2.989892870544796e-157]
[null,"CO2",2.177801997555004e-152,2.19072721740723e-152,2.227258234617236e-152,2.268724620323802e-152,2.316136677027765e-152,2.370771500812413e-152,2.434260888722801e-152,2.508711445625675e-152,2.596860202081579e-152,2.702239057214281e-152,2.829181820687281e-152,2.981861290911477e-152,3.158165286735777e-152,3.312019999418487e-152,3.060269167721929e-152,7.122994831565123e-153,4.352463224385653e-155]
[null,"H2S",1.390686592934676e-152,1.399895126416754e-152,1.427705355754584e-152,1.462005440819918e-152,1.504401783211919e-152,1.557055972633858e-152,1.62295544083425e-152,1.706362371424606e-152,1.813594519798458e-152,1.954462233141069e-152,2.145097621559551e-152,2.413981292575001e-152,2.815832092382813e-152,3.462624045533265e-152,4.463600471879578e-152,2.211784461807632e-152,3.049833206141618e-154]
[null,"C1",75.69759668402565,75.76679732073825,75.89637926642212,75.93132789363352,75.8506884986065,75.62647400897137,75.22002944095686,74.57588659562181,73.61083010413047,72.19318122880085,70.10033139581505,66.92244396677346,61.81339110876714,52.7311317319608,33.96346687494333,4.352980442405896,0.01391403552501578]
[null,"C2",10.8262429228477,10.87665888773248,11.02885774945453,11.21756663988513,11.45267905448049,11.74738931603676,12.11973475172593,12.59512532423407,13.21068073791181,14.0230564132731,15.12341175146213,16.66782815562739,18.94106361110298,22.4564783955894,27.07756309478862,11.50271463551214,0.1355733669609778]
[null,"C3",5.804229398899961,5.809550186946582,5.834731302793185,5.880491270970833,5.953086233594906,6.060954435525509,6.215841758398358,6.434732424794748,6.7433426314464,7.182871685905871,7.824178610184036,8.800953884226733,10.39945162176198,13.35327849348094,19.94921155397838,18.1590494023678,0.4991795173139231]
[null,"I-C4",0.6283717075780045,0.6262858029573228,0.6218249843998437,0.6192942446041388,0.6193285183556685,0.6227733086899351,0.6307961496606996,0.6450810082277394,0.6681862503388877,0.704250260908507,0.7605103741636474,0.8509806877029109,1.006948098885769,1.315240880046478,2.122514509587829,3.267169371901814,0.1653964329245185]
[null,"N-C4",2.374006453016471,2.362968964137328,2.33788024581292,2.320218089777581,2.312348947570469,2.317410422379863,2.339725382758523,2.385527001042521,2.464299043265577,2.59142969000452,2.793956816806801,3.124589918655409,3.702223223969238,4.86311218571244,8.025781765054139,15.03039002255726,0.9572516339972772]
[null,"I-C5",0.7316849754659221,0.7244944752660317,0.7066277700774601,0.6908239778925231,0.6777362477518509,0.6681998048288615,0.6633330680268348,0.6647173739287346,0.674732972477142,0.6972307919434756,0.7390018636526126,0.8134122003214719,0.951123269476928,1.241663649683135,2.099597675831925,6.437373932643974,0.7674197840845896]
[null,"N-C5",0.8589455704549144,0.8493236711940346,0.8252540596507962,0.8036407095596366,0.7852302087334501,0.7709669548846502,0.7621050800117599,0.7604081060853171,0.7685230333599784,0.7907294835107439,0.8345811148382398,0.914975088567385,1.066196994299921,1.388942573586057,2.357290567541327,8.205144897536542,1.160052222321046]
[null,"C6",0.9276349925521544,0.9118339013647189,0.8718429143599107,0.8349553196474621,0.8018843873419963,0.7734853922881058,0.7508490585353643,0.735470502913161,0.7295676059490703,0.7367203835145278,0.763275893472208,0.8218479699609976,0.9417645853125705,1.210546791105062,2.058514135499822,11.29377322835707,3.154254753651597]
[null,"C7",0.6702562971473534,0.6546119726475247,0.6149674101206362,0.5782031297839743,0.5447512604322554,0.5150936030169467,0.4898117780324404,0.4696787326811545,0.4558309857735124,0.450113164275483,0.4558327252186817,0.4796386685348077,0.5371421079882426,0.6753801678349717,1.130486499247227,8.931396657369502,5.137017573819612]
[null,"C8",0.6139792471412666,0.5953073490823507,0.5481861205288496,0.5046928280310762,0.4651331182073336,0.4298062399686438,0.3990398416069543,0.3732525674789198,0.3530691533926963,0.3395458245349888,0.3346569292648848,0.3424970129874129,0.3728674742062677,0.4556254557946074,0.7422503295559751,7.401707878247652,8.701869220760196]
[null,"C9",0.3111525813746941,0.2994619595065002,0.2701886558586558,0.2434697189165692,0.2193927733108534,0.1980184446528023,0.1793962045301083,0.163590597362939,0.1507260563227934,0.1410699730245343,0.1352059826941943,0.1344545432774927,0.1421186613306955,0.1684554161616862,0.2659096242923402,2.997113664017208,7.136534500405997]
[null,"C10",0.1939089292181477,0.1852320179205206,0.1637179393543852,0.1443666522206286,0.1271694574830458,0.112088672467984,0.099068619244314,0.08805125114771248,0.0789995522415365,0.07193672927178175,0.06702293997479665,0.06473579360360675,0.0663984726248216,0.07627784653961098,0.1164203913163289,1.374904574686312,6.571593479948155]
[null,"C11",0.1145000384003925,0.1085579213881116,0.0939864624195877,0.08109607167374062,0.06982761708243035,0.06010015672450952,0.05181918723712713,0.04488660029086035,0.03921334991586237,0.03473785059287084,0.03145868473396546,0.02950801940912679,0.02936289969823484,0.03268023328885924,0.04817927312750912,0.569891272253259,5.423984026286976]
[null,"C12",0.07038314229705422,0.06623153212278476,0.05616982333311232,0.04742607052216648,0.03991865141532362,0.03355188627163939,0.02822267413023346,0.02382746315776777,0.02026981523207745,0.01746973613227367,0.01537832386397165,0.01400873988468085,0.01352383932853941,0.01458123078281602,0.02075567804656406,0.23992015603226,4.51150718895672]
[null,"C13",0.05573886563474819,0.05206021124573903,0.04325276206451849,0.03573950012431153,0.02940929484772246,0.02414175508203267,0.01981390918868884,0.01630645736211902,0.01350964291562869,0.01132936113236214,0.009695470298802477,0.008578303371873732,0.008035049347332656,0.008393003235563461,0.01153415254212261,0.1286383282704009,4.743684339880871]
[null,"C14",0.03672669190859165,0.03404856596330848,0.02771586733943992,0.02241516677355629,0.01803513721052809,0.01446157367290253,0.01158269607513942,0.009293613342148632,0.007499958019530142,0.006121024069632354,0.005093389831059331,0.00437783044376422,0.003979291381161777,0.00402748837925974,0.005343926745060236,0.05713739758296871,4.10251595894705]
[null,"C15",0.0266637623792361,0.02453748382745194,0.01957250434571052,0.015495665781915,0.01219288047881704,0.009552050025434926,0.007467409780914668,0.005842790309041639,0.004593851255398834,0.003649555539339154,0.00295350074992215,0.002466626703698584,0.00217622353808537,0.002134627258235567,0.002735160652408611,0.0279496499448706,3.880145084369593]
[null,"C16",0.01633133894356725,0.01491931058044136,0.01166349369136302,0.009041205504644193,0.006958738845130833,0.005327332519733393,0.004065948503042049,0.003103064095719129,0.002377584725283596,0.001839100285209351,0.001447861559457577,0.00117521954345564,0.001006663119183067,0.0009572038248038255,0.00118470166559989,0.01155425027597879,3.079437741919886]
[null,"C17",0.01177649656263558,0.01068044229895521,0.008184877844665785,0.006213411713095275,0.004678807135213335,0.003501077697031607,0.002609370982689633,0.001942902199919445,0.001451096246639661,0.001093166999968755,0.0008374324542098914,0.0006608253717804198,0.0005497158539288436,0.0005068551286705408,0.000606121726676029,0.005639248121631654,2.865963109848031]
[null,"C18",0.009000279945727796,0.008104121601518527,0.006089182105112723,0.004527840076675658,0.003336547095400428,0.002440941709738987,0.001776990001073883,0.001291226807775595,0.0009403038466577792,0.0006900863834979149,0.0005145596590806373,0.000394864413026896,0.0003190945752547437,0.0002853828111997668,0.0003298538088998748,0.002927586811230582,2.817373260913236]
[null,"C19",0.006304867326760215,0.005636835802739074,0.00415346857932301,0.00302591605439285,0.00218258189256273,0.001561481153355622,0.001110646878575852,0.0007878061183646181,0.0005595430362038058,0.0004001713967491241,0.0002905250758060555,0.0002168759052157061,0.0001703125579016213,0.000147797543938382,0.0001651732086515413,0.001398834038910043,2.531114281766343]
[null,"C20",0.004023017727608935,0.003571514389834488,0.002581306476542394,0.00184287282845023,0.001301424780328604,0.0009107516301883547,0.0006330896201298692,0.000438484142438897,0.0003038371713442311,0.0002118164328254444,0.0001497737328981809,0.0001087967695371271,8.305331060648937e-05,6.995795597450809e-05,7.562203909318056e-05,0.0006113249017959629,2.066059574195874]
[null,"C21",0.002922461423253224,0.002576455929313705,0.001826892387861636,0.00127843030746963,0.0008841295208770326,0.0006053727392280251,0.0004113688668161836,0.0002782841087956232,0.0001881813101753722,0.0001279188679945296,8.812253478354307e-05,6.231070652054634e-05,4.625482287331783e-05,3.783131546171671e-05,3.957045446629671e-05,0.000305485137268713,1.915396726150671]
[null,"C22",0.002102632715620993,0.001840966409353424,0.001280967380225906,0.0008788550717664591,0.0005953682812166668,0.0003989703186927512,0.0002651071186564702,0.000175219464462721,0.0001156681132556431,7.669366689038156e-05,5.14923397874014e-05,3.545472200867716e-05,2.56028766050551e-05,2.03410265572702e-05,2.059652421103639e-05,0.0001519326193721618,1.754828360357236]
[null,"C23",0.001524291644467855,0.001325537499984106,0.0009052712680357649,0.0006090772161374828,0.0004042743997433268,0.0002652108049466239,0.0001723703044934444,0.0001113400353340509,7.177205673425318e-05,4.643268657501339e-05,3.039329024809531e-05,2.03849763330157e-05,1.432505288623431e-05,1.105932650513284e-05,1.084491960175058e-05,7.648020874559336e-05,1.616367459846836]
[null,"C24",0.001099989492812601,0.0009501392292385756,0.0006370333348655499,0.00042040839610501,0.0002734760260896923,0.0001756750310602129,0.0001117106150056549,7.054087520111168e-05,4.441746615208613e-05,2.80470626110623e-05,1.790445232688839e-05,1.170172798200664e-05,8.005156775552239e-06,6.007894788267926e-06,5.708044039226613e-06,3.850610392877438e-05,1.479109225315776]
[null,"C25",0.0008180169080589312,0.0007018931524523746,0.0004620966097143978,0.0002992012801678177,0.0001907955170506519,0.0001200478623052747,7.470992911421646e-05,4.613334816981797e-05,2.838414345078304e-05,1.749925696883258e-05,1.089843124183794e-05,6.943307631918767e-06,4.625766122743146e-06,3.376202576304754e-06,3.109220903592747e-06,2.007556767207046e-05,1.39178931660898]
[null,"C26",0.0006072538521717522,0.0005176340883453547,0.0003347083752622036,0.0002126773152298782,0.0001329819044814985,8.197687518890524e-05,4.994349353334847e-05,3.016733618396404e-05,1.814193577468874e-05,1.092401534076074e-05,6.639703451436419e-06,4.124987243001568e-06,2.677335247511922e-06,1.901144354376336e-06,1.697819259964765e-06,1.049895009518672e-05,1.304759311832522]
[null,"C27",0.0004578294357275004,0.000387733773967965,0.0002462936589733675,0.000153614796127606,9.42062427002107e-05,5.691239191042447e-05,3.395321824546923e-05,2.006735875546989e-05,1.179938433521258e-05,6.941545483865643e-06,4.119025173509642e-06,2.496298373422648e-06,1.579077619218471e-06,1.091331873521413e-06,9.4553927474594e-07,5.603157132727022e-06,1.239964650764353]
[null,"C28",0.0003414422351270098,0.0002873156257695295,0.0001793295934654671,0.0001098149483396325,6.606858410872035e-05,3.912634648644105e-05,2.286418977732246e-05,1.322662796941171e-05,7.606422000990194e-06,4.37342635796537e-06,2.534458218471977e-06,1.498909351612192e-06,9.244360749157181e-07,6.220840006827748e-07,5.23138751031851e-07,2.972632392175236e-06,1.163220437300526]
[null,"C29",0.0002548080384888982,0.0002130600610637583,0.0001306968789110658,7.859751629787624e-05,4.640243471848152e-05,2.694515783543306e-05,1.542783999437723e-05,8.738055226275432e-06,4.916399808800745e-06,2.763622666351682e-06,1.56465733705186e-06,9.033509535534259e-07,5.433989566056673e-07,3.561932871009255e-07,2.908673966166854e-07,1.585835640762591e-06,1.089691782832687]
[null,"C30+",0.0004130134056631852,0.0003248155159812178,0.0001685434800241243,8.512717633398161e-05,4.191043674581361e-05,2.015227435672646e-05,9.488538584011526e-06,4.389444914167308e-06,2.003793840960232e-06,9.079159896209795e-07,4.116010097557467e-07,1.889583783512114e-07,8.96400861277737e-08,4.577604868716281e-08,2.827228747602821e-08,1.039512527063344e-07,16.62303164019291]
[null,"Total",99.99999999999997,99.99999999999999,100,99.99999999999997,99.99999999999999,100,100,100,100,99.99999999999997,100,100,100,99.99999999999997,100,99.99999999999997,99.99999999999999]

{"sheet":"4-DLE-plots","index":9,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[null,"Figure 2: Plots Differential Liberation Expansion (DLE)"]
[]
[null,null,null,"(A) Solution Gas Oil Ratio",null,null,null,null,"(B) Relative Oil Volume"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(C) Oil Density",null,null,null,null,"(D) Gas Z Factor"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(E) Incremental Gas Gravity (air = 1)"]

{"sheet":"5-Sep-Test","index":10,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[31,5,31,8],[31,1,31,4],[33,1,33,4],[20,7,20,8],[33,6,33,9],[20,2,20,4]]}
[null,"5. Separator Test"]
[]
[null,"Table 11: Multi-stage Separator Test"]
[null,"The multi-stage separator test provides fluid properties such as GOR, density and oil formation volume factor at"]
[null,"separator test conditions"]
[]
[null,null,"Pressure","Temperature","GOR¹","GOR²","Separator Volume Factor³","Specific Gravity Flashed Gas","Oil Density","Stock Tank Oil Gravity"]
[null,null,{"$f":"p_unit_p","v":null},{"$f":"T_unit_p","v":null},{"$f":"sep_gor1_unit_p","v":null},{"$f":"gor_unit_p","v":null},{"$f":"sep_bo_unit_p","v":null},"(air=1)",{"$f":"dens_unit_p","v":null},"(API)"]
[null,"Psat",2875.456564497617,237.716614,0,0,1.46986190452016,"-",41.38650451747259,"-"]
[null,"-",100,99.99999999999999,710.2075278344462,686.5360974627324,1.034479513108193,0.8330390202938519,51.03032527269706,"-"]
[null,"Stock tank",14.696,59.99999999999998,39.78247216555463,39.78247216555463,1,1.251350574349387,52.11309248027182,37.84199162711101]
[]
[]
[]
[]
[null,"¹Volume of gas liberated at standard conditions per volume of stock-tank oil at standard conditions "]
[null,"²Volume of gas liberated at standard conditions per volume of oil at indicated pressure and temperature"]
[null,"³Volume of oil at indicated pressure and temperature per volume of stock-tank oil at standard conditions "]
[]
[null,"Figure 3: Plots Multi-stage Separator Test"]
[null,null,"(A) GOR¹",null,null,null,null,"(B) GOR²"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"             (C) Separator Volume Factor",null,null,null,null,"(D) Specific Gravity of Flashed Gas"]

{"sheet":"5-Sep-Test-Compositions","index":11,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[[2,1,2,19]]}
[null,"Table 12: Compositions from Multi-stage Separator Test"]
[null,"Removed gas compositions mol-%."]
[null,"Notes:\n1. First column is the incipient gas at bubblepoint.\n2. Last column (*) is stock tank oil at standard conditions (1 atm, 60 F)"]
[null,"Pres (psia)",2875.46,100,14.7,"14.7*"]
[null,"N2",4.510563243859107e-152,2.849964964690662e-152,4.440594095710642e-153,6.948552235412659e-156]
[null,"CO2",2.177801997555004e-152,2.686623193365078e-152,2.566887263801412e-152,3.964283800490557e-154]
[null,"H2S",1.390686592934676e-152,2.404381443917856e-152,4.63373312156197e-152,2.194848807924977e-153]
[null,"C1",75.69759668402565,67.90218352992896,27.46933135232426,0.1318760050391677]
[null,"C2",10.8262429228477,16.1978554155809,27.72453493653634,1.066399395420163]
[null,"C3",5.804229398899961,9.578503602715841,26.4297214144784,3.934590465244307]
[null,"I-C4",0.6283717075780045,0.9111536031219204,2.765986572234839,1.082158684290361]
[null,"N-C4",2.374006453016471,3.221855087928571,9.789872850436319,5.581662330307039]
[null,"I-C5",0.7316849754659221,0.6894327311811936,1.981122576797173,3.030676440560654]
[null,"N-C5",0.8589455704549144,0.7095900519067657,1.972483067181943,4.089133618313978]
[null,"C6",0.9276349925521544,0.4831292643075518,1.233442514676805,6.887541725258949]
[null,"C7",0.6702562971473534,0.1877510617066863,0.4176533294196695,7.360837101185057]
[null,"C8",0.6139792471412666,0.08675698745101898,0.1664707967522591,9.24411394689032]
[null,"C9",0.3111525813746941,0.02194994371104872,0.03624866442628452,6.285422647792376]
[null,"C10",0.1939089292181477,0.006824235238090445,0.009695325914147079,5.196762039044285]
[null,"C11",0.1145000384003925,0.002015076345547839,0.002463263322125921,4.043113780913847]
[null,"C12",0.07038314229705422,0.0006219059246593585,0.0006544076111114615,3.25767699317954]
[null,"C13",0.05573886563474819,0.0002484125341438017,0.0002251400911252339,3.367229918195708]
[null,"C14",0.03672669190859165,8.296445507991088e-05,6.480693354000657e-05,2.885139730609393]
[null,"C15",0.0266637623792361,3.069086871684052e-05,2.067902602693705e-05,2.714731964144453]
[null,"C16",0.01633133894356725,9.633222992669254e-06,5.603777936352051e-06,2.148237746834677]
[null,"C17",0.01177649656263558,3.580445020420434e-06,1.799894290633159e-06,1.995918658757162]
[null,"C18",0.009000279945727796,1.419259047539222e-06,6.172255810847917e-07,1.960079742487976]
[null,"C19",0.006304867326760215,5.190894551387061e-07,1.955298206535175e-07,1.759816490151885]
[null,"C20",0.004023017727608935,1.740459742616574e-07,5.685024178108111e-08,1.435899441998557]
[null,"C21",0.002922461423253224,6.688232260973884e-08,1.896813722491303e-08,1.330839203952232]
[null,"C22",0.002102632715620993,2.564219173634009e-08,6.32286194985295e-09,1.219058609039006]
[null,"C23",0.001524291644467855,9.974549737973722e-09,2.141362963611121e-09,1.122734626134624]
[null,"C24",0.001099989492812601,3.890100588393468e-09,7.28127314485435e-10,1.027306669217808]
[null,"C25",0.0008180169080589312,1.575212010526131e-09,2.574507119788455e-10,0.9666001502021102]
[null,"C26",0.0006072538521717522,6.414513378551998e-10,9.168020668212144e-11,0.9061176388792992]
[null,"C27",0.0004578294357275004,2.672551165700391e-10,3.345449842444567e-11,0.8610917689647191]
[null,"C28",0.0003414422351270098,1.109958354023173e-10,1.218837439276685e-11,0.8077775545032747]
[null,"C29",0.0002548080384888982,4.648550973800584e-11,4.485094326861273e-12,0.7567034329874166]
[null,"C30+",0.0004130134056631852,2.920088597829854e-13,8.094755555128212e-15,11.54275147949967]
[null,"Total",99.99999999999997,100,100,100]

{"sheet":"6-CVD","index":12,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,"6. Constant Volume Depletion (CVD)"]
[]
[null,null,"Table 13: Constant Volume Depletion at Reservoir Temperature"]
[null,null,"Pressure","Oil Saturation","Relative Moles Removed","Gas Z Factor","Gas Gravity","Gas Viscosity","Oil Viscosity"]
[null,null,null,"Vliq/Vtot",null,"Z"]
[null,null,{"$f":"p_unit_p","v":null},"(%)","(%)","-","-",{"$f":"visc_unit_p","v":null},{"$f":"visc_unit_p","v":null}]
[null,"Psat",2875.456564497617,100,0,0.8491571785774881,0.8392414433853175,0.02207961876596794,0.3255769851515713]
[null,null,2800,99.13070599109984,0.960457854475727,0.8478525941733578,0.8352452781627223,0.02159903593673405,0.333566494760603]
[null,null,2600,96.9213550009579,3.63843395366672,0.8454913855200504,0.8257574493813872,0.0203909821868511,0.3559037810946501]
[null,null,2400,94.82440182523302,6.512568612727887,0.84471340435361,0.8179262066759603,0.01928015126190276,0.3801416399856636]
[null,null,2200,92.81935270467827,9.585453383444287,0.8455088071818754,0.8118562534876759,0.01826762425183006,0.4065512179369346]
[null,null,2000,90.88887523832487,12.85807897723117,0.8478638789010569,0.8077183337340653,0.01735283748177832,0.4354450083979625]
[null,null,1800,89.01773712936075,16.33017090582599,0.851760310078408,0.8057800304625139,0.01653319745136985,0.4671885978770617]
[null,null,1600,87.19174536161616,20.00089502823188,0.857175470980301,0.8064591225198675,0.01580385625178068,0.502219532993711]
[null,null,1400,85.39647781435488,23.87015307566697,0.8640840972566114,0.8104200939573878,0.01515756516272785,0.5410799054588222]
[null,null,1200,83.61543809379373,27.94092137250306,0.8724621867472863,0.8187598190701005,0.01458442797072647,0.5844771439704219]
[null,null,1000,81.82681085602276,32.22370761315459,0.882295082907766,0.8333956495660231,0.01407118121705645,0.6334081160070868]
[null,null,800,79.9966081335765,36.74606856671163,0.893595671653392,0.8579719424482656,0.01359911403258262,0.6894437719458912]
[null,null,600,78.0609141023119,41.57687458439074,0.9064547223590951,0.9003329716557817,0.01313802072612831,0.7555001073344384]
[null,null,400,75.86492868652134,46.90747712161426,0.9212356219205746,0.9810357463182328,0.01262623387269592,0.8385595803012542]
[null,null,300,74.62827348257825,49.8154249968965,0.9291597940092062,1.057347273368836,0.01229890317556821,0.8891874279907074]

{"sheet":"6-CVD-Compositions","index":13,"n_rows":39,"n_cols":18,"rows_kept":39,"cut":false,"hidden":false,"merged":[]}
[null,"Table 14: Compositions from Constant Volume Depletion (CVD) Test"]
[null,"Removed gas compositions, mol-%. *Residual oil at last CVD stage"]
[null,"Pres (psia)",2875.46,2800,2600,2400,2200,2000,1800,1600,1400,1200,1000,800,600,400,300,"300.0*"]
[null,"N2",4.510563243859107e-152,4.478467829324267e-152,4.383029359001709e-152,4.268128982860342e-152,4.132543212671541e-152,3.974907386383019e-152,3.793622031963194e-152,3.586706590492924e-152,3.351565649986164e-152,3.084601259909384e-152,2.780534552830623e-152,2.431129197614792e-152,2.0225544443697e-152,1.529339799210766e-152,1.194902892562626e-152,3.966726846409502e-154]
[null,"CO2",2.177801997555004e-152,2.19072721740723e-152,2.226821401688372e-152,2.266478612098146e-152,2.310300045080451e-152,2.359006012598369e-152,2.413458358815724e-152,2.474677266980387e-152,2.543830161148654e-152,2.622123701288029e-152,2.710377000398353e-152,2.807494903965831e-152,2.904653634814319e-152,2.958902312956948e-152,2.935442752471932e-152,3.526838994815347e-153]
[null,"H2S",1.390686592934676e-152,1.399895126416754e-152,1.427457921502822e-152,1.460706928755366e-152,1.500958999481808e-152,1.549960849612873e-152,1.610085092362351e-152,1.684647145656922e-152,1.778439804688145e-152,1.898680277963972e-152,2.056784241572291e-152,2.271890045292315e-152,2.5781147186897e-152,3.036857645731284e-152,3.39039634579361e-152,8.691481311232968e-153]
[null,"C1",75.69759668402565,75.76679732073825,75.89795778433304,75.94051980067344,75.87680082825511,75.68313248060942,75.32692785599852,74.7617722046348,73.91879153643187,72.69053191009553,70.89846778170205,68.2207327287874,64.00885652846836,56.73250230543078,50.31983262513086,3.341098620005424]
[null,"C2",10.8262429228477,10.87665888773248,11.02733603031536,11.20941882728476,11.43073677459958,11.7015634832742,12.0356790590237,12.45205783846713,12.97765405895454,13.65219364918524,14.5367664946218,15.72966920497697,17.39396500770795,19.77186280709289,21.51236378967498,4.697706855890827]
[null,"C3",5.804229398899961,5.809550186946582,5.834443667474559,5.878759421767142,5.948042133341085,6.049766854425091,6.194302874728581,6.396543837748945,6.678812967502834,7.076379018880798,7.648789274437521,8.505641998056749,9.873585655329469,12.30354755233411,14.4906290878711,6.848368346954794]
[null,"I-C4",0.6283717075780045,0.6262858029573228,0.6218306477366613,0.6192867854113587,0.6192345465555316,0.6224543265644691,0.630029727361204,0.6435257014070915,0.6653137313083228,0.6992068886023938,0.7518115150611907,0.8357517268936169,0.9786809256933547,1.255099634822757,1.520824267985521,1.246725869824954]
[null,"N-C4",2.374006453016471,2.362968964137328,2.337920645515715,2.32028809390774,2.312255857968416,2.316757036838248,2.337863440437315,2.381463453357511,2.45650699190197,2.577453606322339,2.769527210312887,3.08139394476479,3.62119342743319,4.687575442498121,5.728642449280801,5.820448168906482]
[null,"I-C5",0.7316849754659221,0.7244944752660317,0.7066637035223602,0.6909545949291697,0.6779704161289215,0.6685014607720294,0.6636236547701222,0.6648728599446635,0.6745699370839254,0.6964693295042437,0.7371734650622964,0.8096143727285531,0.9432420620663637,1.223010422914986,1.506097770434107,2.696789870286398]
[null,"N-C5",0.8589455704549144,0.8493236711940346,0.8252989361531687,0.8038063009933741,0.7855350748757145,0.7713809836845992,0.7625557663376293,0.7607818748626878,0.768656894654573,0.7903827666194549,0.833360593884642,0.9121302278548568,1.059958645315472,1.373585663880299,1.693244225831525,3.546757057760237]
[null,"C6",0.9276349925521544,0.9118339013647189,0.871893879761568,0.8351434665445249,0.8022369997064558,0.7739894121951781,0.751467435737002,0.7361554902577263,0.7302704145697827,0.7373965350305839,0.7638842981456478,0.8223350160034247,0.9419862703588235,1.209763333110116,1.489679428991748,5.844618120830851]
[null,"C7",0.6702562971473534,0.6546119726475247,0.6149977584949456,0.5783081700390746,0.5449353921411895,0.5153388363580065,0.4900922209306325,0.4699720718980291,0.4561277552155014,0.450425760006283,0.4562086390225259,0.4801896567134671,0.5381273100780873,0.6774962535592084,0.8271955828837706,6.279234500097715]
[null,"C8",0.6139792471412666,0.5953073490823507,0.548208058228111,0.5047602430216452,0.4652345384380332,0.4299145583024654,0.3991267099883613,0.3732983490506337,0.3530697174798086,0.3395185180353024,0.3346503458283082,0.3426163506628916,0.3733562723871377,0.4572003669005783,0.5507514974461738,8.000972522741094]
[null,"C9",0.3111525813746941,0.2994619595065002,0.270195835351821,0.2434859367046526,0.2194045313773932,0.1980077079994746,0.1793474723646585,0.1634948712261612,0.1505826541340026,0.140887461278108,0.1350042043757708,0.1342722041607051,0.1420418874800675,0.168746507485444,0.2001865660316779,5.513768866321164]
[null,"C10",0.1939089292181477,0.1852320179205206,0.163719808741094,0.144365544189292,0.1271532639268812,0.1120449458344091,0.09898844432966632,0.08793079006837509,0.07884007961525327,0.07174400956459756,0.06680694104323889,0.06451256095339608,0.06620029740832407,0.07620515284290055,0.08895177707648001,4.604148415564349]
[null,"C11",0.1145000384003925,0.1085579213881116,0.09398609102427691,0.081089389807582,0.06980606862934727,0.06005650829598554,0.05174931899812591,0.04478980018264939,0.03909173544870453,0.03459545744567803,0.03130069904355708,0.02934081149162181,0.02919697362161281,0.03254855605564046,0.03736760401709708,3.606309503595428]
[null,"C12",0.07038314229705422,0.06623153212278476,0.05616877419606669,0.04741877884442398,0.03989942640955533,0.03351673633861845,0.02817002807127586,0.02375796375719346,0.02018564920200049,0.01737384644313023,0.01527374259389503,0.01389826887575262,0.01341077601064195,0.01447580901919947,0.01634302435323575,2.918714686878475]
[null,"C13",0.05573886563474819,0.05206021124573903,0.04325136407344991,0.03573164008579809,0.02939039867142653,0.02410921641622661,0.01976732649959325,0.0162471775555993,0.01344003036978599,0.01125206683667654,0.009612849359610657,0.008492064245611899,0.007946392984194507,0.008305459308189253,0.009220804492624093,3.025699509218751]
[null,"C14",0.03672669190859165,0.03404856596330848,0.02771462818137251,0.02240888322002269,0.01802088432698621,0.0144380687068214,0.01155022646588107,0.009253560183973979,0.007454214522535286,0.006071482103802686,0.005041565083429764,0.004324635079875822,0.003925007622328417,0.003972796813239966,0.004337486875763971,2.597491150601198]
[null,"C15",0.0266637623792361,0.02453748382745194,0.01957141176447212,0.01549047455084588,0.01218159870997029,0.009534080834713632,0.007443334933801221,0.005813912197516213,0.004561719817456796,0.003615594095868094,0.002918761032454151,0.002431653738448397,0.002141018502971685,0.002099065507697314,0.002253951757899817,2.447184186585385]
[null,"C16",0.01633133894356725,0.01491931058044136,0.01166272711370627,0.009037730211749263,0.006951442076697443,0.005316052237558044,0.004051244410869628,0.003085878758203126,0.002358934469075169,0.00181985527629918,0.001428619993607135,0.001156251164814698,0.0009878962267102337,0.0009383783247083809,0.0009911237490902703,1.938169101854516]
[null,"C17",0.01177649656263558,0.01068044229895521,0.008184267814882079,0.006210745954157311,0.004673372094205656,0.003492896765053875,0.002598974014915737,0.001931046457606468,0.001438536975619854,0.001080510950770172,0.0008250676430811321,0.0006489012374181159,0.00053814717442489,0.0004953967844439252,0.0005147507095377151,1.801782846025024]
[null,"C18",0.009000279945727796,0.008104121601518527,0.00608868058064636,0.004525714065997852,0.003332323705611583,0.002434738483657318,0.001769292588288274,0.001282654588265898,0.0009314344617934144,0.0006813560713723127,0.0005062262347836477,0.0003870078428540917,0.0003116312082114335,0.0002781106387830111,0.0002843322892026805,1.770128178256683]
[null,"C19",0.006304867326760215,0.005636835802739074,0.004153097476387338,0.003024383429725383,0.002179608317316747,0.001557212663715888,0.001105469686420161,0.0007821711847345383,0.0005538459430676872,0.0003946926310040698,0.0002854158533990047,0.0002121687700650824,0.0001659386344611485,0.0001436150700364025,0.0001444944540072102,1.589706715704166]
[null,"C20",0.004023017727608935,0.003571514389834488,0.002581059680213393,0.001841876819908329,0.001299534169935115,0.0009080961815874325,0.0006299389692712013,0.0004351307695814948,0.0003005230763857487,0.0002087021152169624,0.0001469364360491488,0.000106242998931982,8.073371683574207e-05,6.778487411908477e-05,6.712800424930409e-05,1.297348742226258]
[null,"C21",0.002922461423253224,0.002576455929313705,0.001826707409162139,0.001277699174702682,0.0008827699752090312,0.0006035026876613251,0.0004091970149303016,0.0002760226357399608,0.0001859959525608461,0.0001259118043727524,8.633611297284151e-05,6.074009546591384e-05,4.486097359367175e-05,3.655348616398284e-05,3.563698187873684e-05,1.202588453306039]
[null,"C22",0.002102632715620993,0.001840966409353424,0.001280831119504497,0.0008783267113750969,0.0005944048405870735,0.0003976715988470619,0.0002636299439450607,0.0001737141018432274,0.000114245313895537,7.541632887889342e-05,5.038150587219108e-05,3.450077650098388e-05,2.477593623252953e-05,1.959974665306202e-05,1.881552852695747e-05,1.101686247170275]
[null,"C23",0.001524291644467855,0.001325537499984106,0.0009051707344462774,0.0006086942886424831,0.0004035891556935709,0.0002643050645775171,0.000171360967944964,0.0001103330411696316,7.084094584730241e-05,4.561543127162573e-05,2.969881005463276e-05,1.980244447323377e-05,1.383188247048575e-05,1.062730257042489e-05,1.004770222487078e-05,1.014706853804202]
[null,"C24",0.001099989492812601,0.0009501392292385756,0.0006369598451063418,0.0004201331539396006,0.0002729923597762992,0.0001750478879967918,0.0001110256548429624,6.987167052876208e-05,4.381198045409041e-05,2.752738641634356e-05,1.747288363755357e-05,1.134812128133178e-05,7.71281162476365e-06,5.757716049909087e-06,5.362445814638627e-06,0.9285075367153234]
[null,"C25",0.0008180169080589312,0.0007018931524523746,0.0004620414541620261,0.0002989979931091063,0.0001904445520926507,0.0001196012682127457,7.423172588729983e-05,4.56757096186014e-05,2.797888102990837e-05,1.715906640830776e-05,1.062229538577117e-05,6.722278491456292e-06,4.447311859104833e-06,3.227051084884754e-06,2.961275324943233e-06,0.8736714062503118]
[null,"C26",0.0006072538521717522,0.0005176340883453547,0.00033466717508606,0.0002125277856051579,0.0001327281680646292,8.165991899917236e-05,4.961066781658976e-05,2.985526934403863e-05,1.787139972605816e-05,1.070186106449751e-05,6.46341859541672e-06,3.987120961806824e-06,2.56862602154958e-06,1.812415815432198e-06,1.639020179529161e-06,0.8190257539215999]
[null,"C27",0.0004578294357275004,0.000387733773967965,0.0002462624768852823,0.0001535032993921359,9.402021922729509e-05,5.6684214869878e-05,3.371819312668393e-05,1.985140306511348e-05,1.16160684826223e-05,6.794259082431141e-06,4.004746340789012e-06,2.408961689190329e-06,1.511813465287279e-06,1.037719842451555e-06,9.250226867343341e-07,0.7783430777683552]
[null,"C28",0.0003414422351270098,0.0002873156257695295,0.0001793062936136925,0.0001097328338169253,6.593384171221195e-05,3.896401361529637e-05,2.270013990464844e-05,1.307887200764253e-05,7.483583124412152e-06,4.276837386386189e-06,2.461164619498244e-06,1.444161190638773e-06,8.832451208237527e-07,5.900228352156907e-07,5.185393013749205e-07,0.7301630275954185]
[null,"C29",0.0002548080384888982,0.0002130600610637583,0.0001306794845918457,7.85370750603814e-05,4.630486638562068e-05,2.682967682542977e-05,1.53133136754853e-05,8.636922601600726e-06,4.834035973468025e-06,2.700227403449472e-06,1.517599842578357e-06,8.689874186444248e-07,5.181377159090527e-07,3.36990222389739e-07,2.920548825237206e-07,0.6840038705670539]
[null,"C30+",0.0004130134056631852,0.0003248155159812178,0.0001685164735672615,8.504522797806002e-05,4.179759591502897e-05,2.003988687285978e-05,9.395732123124972e-06,4.321815019000249e-06,1.958700089750611e-06,8.797030232197517e-07,3.946909452043023e-07,1.790502985331219e-07,8.383287369519556e-08,4.228054098789769e-08,3.208770498792051e-08,10.43413193677125]
[null,"Total",99.99999999999997,99.99999999999999,100,100,100,100,100,100,99.99999999999997,100,100,99.99999999999999,99.99999999999997,100,99.99999999999997,100]

{"sheet":"6-CVD-Plots","index":14,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
[null,"Figure 4: Plots for Constant Volume Depletion (CVD)"]
[]
[null,null,null,"(A) Oil Saturation",null,null,null,null,"(B) Relative Moles Removed"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(C) Gas Z Factor",null,null,null,null,"(D) Gas Gravity"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"(E) Gas Viscosity",null,null,null,null,"(F) Oil Viscosity"]

{"sheet":"7-Visc","index":15,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[]}
[null,"7. Viscosity Test (DLE)"]
[]
[null,"Table 15: Viscosity Test at Reservoir Temperature"]
[]
[null,null,"Pressure","Oil Viscosity","Gas Viscosity"]
[null,null,{"$f":"p_unit_p","v":null},{"$f":"visc_unit_p","v":null},{"$f":"visc_unit_p","v":null}]
[null,null,6600,0.5360434501724228]
[null,null,6400,0.5248022832276478]
[null,null,6200,0.5135478442787217]
[null,null,6000,0.5022812015234231]
[null,null,5800,0.4910034539447519]
[null,null,5600,0.4797157301790291]
[null,null,5400,0.4684191869452471]
[null,null,5200,0.45711500693965]
[null,null,5000,0.4458043960776226]
[null,null,4800,0.4344885799372938]
[null,null,4600,0.4231687992242734]
[null,null,4400,0.4118463040322402]
[null,null,4200,0.4005223466168016]
[null,null,4000,0.3891981723257738]
[null,null,3800,0.3778750082322041]
[null,null,3600,0.3665540488889868]
[null,null,3400,0.3552364384545507]
[null,null,3200,0.3439232482116942]
[null,null,3000,0.3326154481930592]
[null,null,2875.456564497617,0.3255769851515713]
[null,null,2800,0.333566494760603,0.02159903593673405]
[null,null,2600,0.3559204541444475,0.02039111257103594]
[null,null,2400,0.3801870733477909,0.01928095336518344]
[null,null,2200,0.4065837170189503,0.01826967871134437]
[null,null,2000,0.4353551947097626,0.01735653148858211]
[null,null,1800,0.4667815935799872,0.01653856821642182]
[null,null,1600,0.5011914443567663,0.01581049058178865]
[null,null,1400,0.5389855015036841,0.01516451871973084]
[null,null,1200,0.5806830479288277,0.01459010421899391]
[null,null,1000,0.6270205144185869,0.01407306363848553]
[null,null,800,0.679188330465234,0.01359312529859558]
[null,null,600,0.7395101755297332,0.01311692256048458]
[null,null,400,0.8140481891857928,0.01257535037289346]
[null,null,200,0.9300159967514466,0.01176980286425217]
[null,null,14.69594300599296,1.568106724633896,0.009732004619471603]
[null,null,14.69594300599296,2.92245597248489]

{"sheet":"7-Visc-plots","index":16,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[null,"7. Viscosity Test (DLE)"]
[null,"Figure 5: Plots for Viscosity Test at Reservoir Temperature"]
[null,null,null,null,null,"Oil Viscosity"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Gas Viscosity"]

{"sheet":"UNITS","index":17,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["T_unit","F",{"$f":"_xlfn.CONCAT(\"(\",B1,\")\")","v":null}]
["p_unit","psia",{"$f":"_xlfn.CONCAT(\"(\",B2,\")\")","v":null}]
["dens_unit","lbm/ft3",{"$f":"_xlfn.CONCAT(\"(\",B3,\")\")","v":null}]
["gor_unit","scf/bbl",{"$f":"_xlfn.CONCAT(\"(\",B4,\")\")","v":null}]
["ogr_unit","STB/1e6scf",{"$f":"_xlfn.CONCAT(\"(\",B5,\")\")","v":null}]
["rg_vol_unit","scf",{"$f":"_xlfn.CONCAT(\"(\",B6,\")\")","v":null}]
["ro_vol_unit","bbl",{"$f":"_xlfn.CONCAT(\"(\",B7,\")\")","v":null}]
["surface_oil_vol_unit","STB",{"$f":"_xlfn.CONCAT(\"(\",B8,\")\")","v":null}]
["visc_unit","cp",{"$f":"_xlfn.CONCAT(\"(\",B9,\")\")","v":null}]
[]
["comp_unit",{"$f":"_xlfn.CONCAT(\"1E-6/\",p_unit)","v":null},{"$f":"_xlfn.CONCAT(\"(\",B11,\")\")","v":null}]
["dle_gor_unit",{"$f":"_xlfn.CONCAT(rg_vol_unit,\"/residual-\",ro_vol_unit)","v":null},{"$f":"_xlfn.CONCAT(\"(\",B12,\")\")","v":null}]
["dle_bo_unit",{"$f":"_xlfn.CONCAT(ro_vol_unit,\"/residual-\",ro_vol_unit)","v":null},{"$f":"_xlfn.CONCAT(\"(\",B13,\")\")","v":null}]
["sep_gor1_unit",{"$f":"_xlfn.CONCAT(rg_vol_unit,\"/\",surface_oil_vol_unit)","v":null},{"$f":"_xlfn.CONCAT(\"(\",B14,\")\")","v":null}]
["sep_bo_unit",{"$f":"_xlfn.CONCAT(ro_vol_unit,\"/\",surface_oil_vol_unit)","v":null},{"$f":"_xlfn.CONCAT(\"(\",B15,\")\")","v":null}]